set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0xa1000448L
mac h: 0x7cdf
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 15.3 seconds (539.4 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0xa1000448L
mac h: 0x7cdf
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 15.3 seconds (539.4 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0xa1000448L
mac h: 0x7cdf
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 15.2 seconds (541.7 kbit/s)...Hash of data verified.
Leaving...com closed
