set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0x34724f6cL
mac h: 0x18fe
get mac res: 1
get flash id : 0x001640c8manufacturer_id: 0xc8

device_id: 0x4016

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 13.5 seconds (610.9 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0x34724f6cL
mac h: 0x18fe
get mac res: 1
get flash id : 0x001640c8manufacturer_id: 0xc8

device_id: 0x4016

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 13.5 seconds (610.9 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0x34724f6cL
mac h: 0x18fe
get mac res: 1
get flash id : 0x001640c8manufacturer_id: 0xc8

device_id: 0x4016

SET FLASH PARAMS

Wrote 1032192 bytes at 0x00000000 in 13.5 seconds (610.1 kbit/s)...Hash of data verified.
Leaving...com closed
